Параметры сцены

Ширина сцены 10(м)

Глубина сцены (от красной линии до задней стены) 9 м

Высота сцены 5 (м)

Рабочая ширина сцены 9 (м)

Рабочая глубина сцены 14 (м)

Ширина зеркала сцены 6 (м)

Высота зеркала сцены 4 (м)

Ширина рабочего зеркала сцены 6 (м)

Высота рабочего зеркала сцены 4,5 (м)

Ширина архитектурного портала 2 (м)

Высота архитектурного портала 5 (м)

Количество штанкетных подъемов 10 (шт.)

Длина штанкета 8 (м)

Сечение штанкета 6см

Расстояние между штанкетами 25см , 50см

Количество софитных ферм 3 (шт.)

Максимальная высота подъема штанкетов 5(м)

Максимальная высота подъема софитных ферм 5 (м)

Количество индивидуальных подъемов 13

Система управления механизацией отдельно по каждому виду оборудования, место расположения пультов - Ручное управление

Stage Details

Stage width - 10 m.

Stage depth (from the setting line to the back wall) – 9 m.

Stage height – 5 m.

Stage working width – 9 m.

Stage working depth – 14 m.

Stage opening width – 6 m.

Stage opening height – 6 m.

Working stage opening width – 6 m.

Working stage opening height – 4,5 m.

Portal width – 2 m.

Portal height – 5 m.

Number of flying bars – 10 pieces.

Flying bars length – 8 m.

Flying bars cross-section – 6 cm.

Distance between flying bars – 25 cm, 50 cm.

Number of light farms – 3 pieces.

Flying bars max. height – 5 m.

Light farms max. height – 5 m.

Number of point hoists – 13 pieces.

Drive mechanism control system for every kind of equipment, location of controls – manual control.